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Please read and keep this instruction manual. Indoor use only!




INTRODUCTION

1. Please read instructions before using this appliance.
2. When using this appliance, basic precautions should always be followed to reduce the risk of fire, electric shock and injury.
3. Clean machine thoroughly before and after all uses following cleaning instructions below.








ELECTRICAL REQUIREMENTS

Wire warmer into a grounded circuit with correct voltage and sufficient power capacity. Refer to the product label (serial plate) on the warmer for voltage and wattage requirements.
All electrical connections must be made according to local codes by a licensed electrician.


ELECTRICAL SPECIFICATION

	Model
	Product Dimension(mm)
	Voltage/Hz
	Watt
	N.W.
G.W.
	Packing Dimension(mm)

	HSW600
	609 x 155 x 73
	240V/50Hz

	500W
	N.W.: 3kg
G.W.: 3.6kg
	655 x 220 x 120

	HSW900
	914 x 155 x 73
	
	850W
	N.W.: 3.5kg
G.W.: 4.2kg
	960 x 220 x 120

	HSW1200
	1219 x 155 x 73
	
	1200W
	N.W.: 5kg
G.W.: 6kg
	1265 x 220 x 120

	HSW1500
	1524 x 155 x 73
	
	1550W
	N.W.: 7kg
G.W.: 8kg
	1600 x 220v120

	HSW1800
	1829 x 155 x 73
	
	1750W
	N.W.: 9kg
G.W.: 10kg
	1850 x 220 x 120




SAFETY INSTRUCTIONS
Warning! All power must be disconnected at power source before any service procedure is performed.
1. This appliance is hot when in use. To avoid burns, do not touch hot surfaces. Keep combustible materials, such as drapes and other furnishings, away from appliance.
2. Never leave the unit unattended while it is working.
3. Always turn the power off at the circuit breaker before cleaning, adjusting or maintaining this machine.
4. Do not operate any appliance after it malfunctions, has been dropped, or damaged. Return appliance to an authorized service facility for examination, electrical or mechanical adjustment, or repair.
5. Do not use outdoors. This appliance is not intended for use in wet or moist locations. Never locate appliance where it may fall into water.
6. To prevent a possible fire, it is recommended that the unit is installed above a non-combustible surface.
8. This appliance has electrical parts. Do not use it in areas where gasoline, paint, or flammable liquids are used or stored.


INSTALLATION

1. Use MOUNTING BRACKET supplied with the warmer. Install with the following clearances:  9” min. between end of unit and any wall, 12” min. between side of unit and any wall, 16” min. between bottom of unit and counter, and 1 7/8” min. between top of unit and overhead surface.
2. This unit radiates heat when in use therefore we recommend that the unit be installed above a non-combustible surface.



OPERATION

For strip warmers of high wattage (18-25 watts per inch), 10-16" is the recommended mounting height.
3. Do not install food warmers above or around combustible surfaces.
4. Food warmers can be mounted to the underside of a shelf with a minimum gap of 1" to protect electrical system.
5. Remove the two center screws from end plates. Align the holes on the bracket with the mounting holes on the end plate. Use the screw to secure the bracket.
6. Drill 4 holes on the underside of a shelf, use fasteners to install the brackets to the underside of the shelf.
7. Place food products in a pan located directly under the warmer for best results.
8. Turn warmer off when not in use.



CLEANING

NOTE: Proper maintenance plays an important part in the life span and functioning of the warmer.
· Turn warmer off before cleaning.
· Do not immerse in water or other liquid. Avoid splashing water into unit.
· The housing and reflectors are made of stainless steel, which can be kept clean by use of a damp sponge and soap solution.
 
TROUBLESHOOTING

	No Heat
	Check that toggle switch is turned “ON”.

	
	Check power at heater.

	Unit Blows Fuse or Circuit Breaker
	Check to make sure circuit is not overloaded.





WIRING DIAGRAM















	S/N
	Description

	1
	Toggle switch

	2
	Heating lamp

	3
	Heating element
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